0x0655 Receive Timeout

Used in: Generic Card Configure (0x0122), Generic Card Query (0x0123), Resource Connect (0x0127), and Resource Query (0x012C) messages.

Byte | Description
0, 1 | Tag: 0x0655 Receive Timeout
2, 3 | Length: 0x0004
4-7 | Value[0-3]: Length of T1, in milliseconds. Normally 35000. 35000 (Default)

Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)