You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Querying Active Ethernet Interface

Querying Active Ethernet Interface

Right-click the DSP-S2 card and select the menu option, Query Active Ethernet Interface.

If redundancy is enabled, then a message will display what port is active.

If redundancy is disabled, then the next dialog opens.

No cables

If there are no cables connected to the DSP-S2 ethernet ports on the I/O card, the next dialog box is displayed:

Digital Signal Processor
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.