You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > ARP Cache Menu

ARP Cache Menu

Description

The ARP cache menus are related to the VDAC-ONE or IP Network Interface Series 2 cards in your system. If you do not have a these cards provisioned, these menus are disabled.

ARP Cache

Viewing ARP Cache

You can view the ARP Cache by doing the following:

1. Right-click a card in the node view.

2. Select ARP Cache Information from the pop-up menu.

3. Select the module for which you want to view the ARP cache.

The Viewing ARP Cache window opens:

Remove all ARP Cache Entries

If you choose the Remove all ARP Cache Entries menu, the CSA sends the ARP Cache Query message with the Remove Entries TLV to the node. This message removes all the entries in the ARP Cache table immediately. Usually the Cache is cleared every five minutes by default.

Remove IP Address / Remove Ethernet Address

The menus clear the entries in the particular VoIP Module that has that IP Address or MAC Address.

Refresh

The Refresh menu causes the CSA to query the node for the ARP Cache information and displays the new values.

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
See Converged Services Administrator.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).