You are here: CSP Hardware Installation and Maintenance > 2 CSP 2090/CSP 2110 Chassis Reference > Environmental Specifications

Environmental Specifications

Specifications

The table below lists the environmental specifications for the CSP 2090 and CSP 2110 chassis.

Characteristic | Specifications
--- | ---
Temperature - Storage | –40~C to + 70~C (–40~F to 158~F)
Temperature - Operating | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | –40~C to +70~C to –40~C (–40~F to 158~F to –40~F) @ 5~/minute
Temperature Shock - Operational | 0~ to 50~ to 0~C (32~F to 122~F to 32~F) at 10~C/hour
Humidity - Operating | 5 to 85%
Altitude | Up to 4000 m (13,123 ft)

Important! Elevated operating ambient conditions may occur in an enclosed equipment rack. If this unit is installed in a closed or multi-unit rack assembly, the operating ambient temperature may be greater than the room ambience.