0x05FF DSP Cache Modify Action

Use this TLV in the DSP Cache Modify message.

Byte | Description
0, 1 | Tag: 0x05FF DSP Cache Modify Action
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Action 0x0000 - Clear Specific Cache (also requires one or more File ID TLVs) 0x0001 - Clear All Caches 0x0002 - Copy Specific Cache (also requires the File ID, File Format, and File Location TLVs)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor