0x10 ISDN Formatted IEs

Used in:
Channel Release Request, Channel Released With Data, Release Channel with Data, Request For Service With Data, Route Control, Outseize Control, PPL Event Indication, PPL Event Request messages

ICB Type | 0x02 (Data)
ICB ID | 0x10
Data Length | Variable
Data[0] | Number of IEs (0–30)
Data[1] | IE 1 Type 0x01 Call Reference 0x02 Called Party Number 0x03 Calling Party Number 0x04 Called Party Subaddress 0x05 Calling Party Subaddress 0x06 Redirecting Number 0x07 Cause 0x08 Progress 0x09 User to User 0x0A Codeset 6 0x0B Codeset 7 0x0C Reserved 0x0D Reserved 0x0E Reserved 0x0F Reserved 0x10 Reserved 0x11 Codeset 5 0x12 Vari-A-Bill
Data[2] | IE 1 Length (0–130)
Data[3] | IE 1 Data[0]
Data[:] | IE n Type
Data[:] | IE n Length (0–130)
Data[:] | IE n Data[0]

RFS. A Status Message indicating that some entity is requesting service from the Excel platform.
Outgoing call setup during real-time call processing on a specific channel.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.