0x09D1 Global Title Group Query Response

Used in:
SS7 SCCP/TCAP Query message

Byte | Description
0, 1 | Tag 0x09D1 Global Title Group Query Response
2, 3 | Length 0x0009 Note: If you attempt to query either a Global Title Group that does not exist, the TLV length in the response will be one byte consisting of null data.
4 | Value[0] State 0 Group Idle 1 Group In Service
5 | Value[1] Stack ID - State this group belongs to.
6 | Value[2] GTI GT Indicator
7 | Value[3] TT Translation Type
8 | Value[4] NP Numbering Plan
9 | Value[5] NAI Nature of Address Indicator
10 | Value[6] Minimum Digits - The minimum number of digits the GT Entry of this group contains
11 | Value[7] Maximum Digits - The maximum number of digits the GT Entry of this group contains
12 | Value[8] Group Attribute Bit 0 - Maximum Match 0 Use minimum match rule for this group 1 Use the maximum match rule for this group (best match rule). Bit 1 - UMTS CG (Not used in current release.) 0 Calling Party address will not be changed when GT translation results are "Route on GT." 1 Calling Party address is changed when GT translation results are "Route on GT." The new calling party address is stored in SSN default parameter table. Bit 2 - ANSI TT4 0 Not TT4 Type 1 TT4 Type If this bit is set, no GT entry can be added to this group. Bit 3 - Remove GT 0 Do not remove GT after a successful translation. 1 Remove GT after a successful translation.

See Signaling System Number Seven.
See Transaction Capability Application Part.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.