You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Recorded Announcement File System Query 0x0102

Recorded Announcement File System Query 0x0102

SwitchKit Name

RecAnnFSQuery

Type

EXS API and SwitchKit API message

Description

Recorded Announcement File System Query 0x0102

This message queries the file system used by the VRAS SIMM’s Flash memory on the DSP-ONE card. In response to this message, the CSP sends a Recorded Announcement File System Report (0x0119).

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

BaseFields Base;

UBYTE Slot;

UBYTE SIMM;

UBYTE reserved19[251];

} XL_RecAnnFSQuery;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE Data[251];

} XL_RecAnnFSQueryAck;

C++ Class

class XLC_RecAnnFSQuery : public XLC_OutboundMessage {

public:

UBYTE getSlot() const;

void setSlot(UBYTE x);

UBYTE getSIMM() const;

void setSIMM(UBYTE x);

};

C++ Class Response

class XLC_RecAnnFSQueryAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x000B) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0102) | 3, 4 | Message Type (0x0102)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status (MSB, LSB)
Number of AEs to follow | 10 | Checksum
AE 0x12 DSP SIMM
: | Checksum

Voice Recorded Announcement System
Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
Digital Signal Processor
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit