You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Conference Deleted 0x004D

Conference Deleted 0x004D

SwitchKit Name

ConferenceDeleted

Type

EXS API and SwitchKit API message

Description

Conference Deleted 0x004D

NOTE: If you are using the DSP Series 2 card, you will receive a Resource Delete Indication 0x0129 message to indicate a conference has been deleted.

This message is sent to the host after a conference on an MFDSP or DSP-ONE card is deleted (for example, all channels in the conference are released and the DSP resource is freed up).

Sent by

CSP

SwitchKit Code

C Structure

typedef struct {

unsigned short ConferenceID;

} XL_ConferenceDeleted;

C++ Class

class XLC_ConferenceDeleted : public XLC_InboundMessage {

public:

unsigned short getConferenceID() const;

void setConferenceID(unsigned short x);

};

Resent in EXS API

This message is resent once after five seconds.

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x0007) | 1, 2 | Length (0x0005)
3, 4 | Message Type (0x004D) | 3, 4 | Message Type (0x004D)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8, 9 | Conference ID | 8 | Checksum
10 | Checksum

Digital Signal Processor
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.