0x38 Query Hard-registered PPL Components

This query will return a list of PPL components from which the specified host is registered to receive PPL Event Indication messages (see Response Data).

Used in:
Multi-Host Configure message

ICB Type | 0x01 (Action)
ICB ID | 0x38
Data Length | 0x04
Data[0–3] | Host ID

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Information Control Block.