You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Recorded Announcement Delete 0x0054

Recorded Announcement Delete 0x0054

SwitchKit Name

RecAnnDelete

Type

EXS API and SwitchKit API message

Description

Recorded Announcement Delete 0x0054

This message deletes all announcements stored on a VRAS SIMM. Deletion of a SIMM takes approximately 30 seconds. The host should wait for an Alarm message of "VRAS Erase Complete" before downloading a new announcement to a SIMM.

Sent by

Host

SwitchKit Code

Configuration

RecAnnDelete (

Node = integer,

Slot = integer,

SIMM = integer,

Reserved = integer,

ForcedFlag = integer);

C Structure

typedef struct {

UBYTE Slot;

UBYTE SIMM;

unsigned short Reserved;

UBYTE ForcedFlag;

} XL_RecAnnDelete;

C++ Class

class XLC_RecAnnDelete : public XLC_OutboundMessage {

public:

UBYTE getSlot() const;

void setSlot(UBYTE x);

UBYTE getSIMM() const;

void setSIMM(UBYTE x);

unsigned short getReserved() const;

void setReserved(unsigned short x);

UBYTE getForcedFlag() const;

void setForcedFlag(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0054) | 3, 4 | Message Type (0x0054)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status (MSB, LSB) 0x0009 DSP Chip Dead When the DSP chip is taken out of service by the system, this response is returned in the NACK. 0x000B File System Conversion in Progress Trying to perform a VRAS function while the flash memory on the SIMM is in the process of file system conversion. 0x000C Defragmentation in Progress Trying to perform a VRAS function while the flash memory on the SIMM is in the process of defragmentation.
Number of AEs to follow
AE 0x12 DSP SIMM
: | Reserved (3 bytes) | 10 | Checksum
: | Checksum

Voice Recorded Announcement System
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Digital Signal Processor
Negative acknowledgement to a message.