0x000E IP Signaling Series 3 Card Interface Service State

Used in:
IP Signaling Series 3 Card Configure message (0x0100)
IP Signaling Series 3 Card Query message (0x0101)

Byte | Description
0, 1 | Tag 0x000E
2, 3 | Length 0x0002
4 | Value[0] State, MSB 0x00
5 | Value[1] State, LSB 0x00 Out of Service 0x01 In Service

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
Most Significant Bit
Least Significant Bit