You are here: PPL Developer’s Guide > 6 SS7 Atomic Functions > L3P TUP (0x0011)

L3P TUP (0x0011)

This section documents the atomic functions associated with L3P TUP.

Atomic Functions

AF Number | 51
--- | ---
Name | Check if segmentation required
Type | Test
Description | Based on the Length of the message and the OFCI/OBCI segmentation indicator, a decision is made if the message has to be segmented.
Arg1 | OFCI/OBCI parameter ID
| 0 : 255
Arg2 | None
| --
Result | PPLevIntEVENT_0 – Msg not segmented PPLevIntEVENT_1 – Msg segmented

TUP Virtual CIC

The following AFs are specific to the L3P TUP Call Control PPL component for TUP Virtual CIC.

AF Number | 73
--- | ---
Type | Normal
Description | Send PPL Event Indication to Host with VCIC AIB
Arg1 | Event Id 1:65535
Arg2 | Not Used

AF Number | 136
--- | ---
Type | Normal
Description | Send channel status change PPL Event Indication to Host with VCIC AIB
Arg1 | OOS flag. 0:1
Arg2 | OOS reason. 0:255

AF Number | 137
--- | ---
Type | Normal
Description | Send PPL Event Request ACK with VCIC AIB
Arg1 | Status. 0:511
Arg2 | Not Used

Telephone User Part
See Atomic Function.
See Circuit Identification Codes.
Setting up, monitoring, and tearing down calls.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Address Information Block.
Out of Service
Positive acknowledgment to a message