0x25 ISDN Segmented Message

Used in:
Outseize Control message
Request For Service With Data message
Release Channel With Data message
Channel Release Request message
PPL Event Indication message
PPL Event Request message
Route Control message

ICB Type | 0x02
ICB ID | 0x25 ISDN Segmented Message
Data Length | 0x02
Data[0] | Number of segments remaining
Data[1] | Segmented ISDN message type

Outgoing call setup during real-time call processing on a specific channel.
RFS. A Status Message indicating that some entity is requesting service from the Excel platform.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
See Integrated Services Digital Network.