# MSP_CHANNEL_ADDR

Creates audio and video MSPP channels for the 3G-324M Interface. MSP_CHANNEL_ADDR is used by mspCreateChannel.

When you use this structure, you must enter a channel type identifier in the channelType field. See Creating a channel for a list of channel type identifiers. You can enable inband DTMF carriage capability for an audio channel by setting the FilterAttribs field to MSP_FCN_ATTRIB_RFC2833.

typedef struct tag_MSP_CHANNEL_ADDR
{
DWORD size;
DWORD nBoard; // Channel location (board number)
MSP_CHANNEL_TYPE channelType;
DWORD FilterAttribs; // Used to enable DSP Filter functions
} MSP_CHANNEL_ADDR;

For more information about mspCreateChannel, see the MSPP Service Developer's Reference Manual.