# MSPP video-enhanced structure categories

This topic categorizes the MSPP video-enhanced structures. Subsequent topics describe each structure in alphabetical order.

## Structures for creating MSPP endpoints

Use the following MSPP video-enhanced structures to create MSPP endpoints:

- MSP_ENDPOINT_ADDR

- MSP_ENDPOINT_PARAMETER

- MUX_ENDPOINT_ADDR

- RTP_PAYLOAD_MAP

- RTPRTCP_ENDPOINT_ADDR

- RTPRTCP_ENDPOINT_PARMS

- RTPRTCP_V6_ENDPOINT_ADDR

- RTPRTCP_V6_ENDPOINT_PARMS

## Structures for creating MSPP channels

Use the following MSPP video-enhanced structures to create MSPP channels:

- MSP_AUDIO_CHANNEL_PARMS

- MSP_CHANNEL_ADDR

- MSP_CHANNEL_PARAMETER

- MSP_VIDEO_CHANNEL_PARMS

## Structures for modifying the 3G-324M Interface configuration

Use the following video-enhanced structures to modify the 3G-324M Interface configuration:

- msp_ENDPOINT_RTPFDX_ENABLE_SKEW_CALC

- msp_ENDPOINT_RTPFDX_H263_ENCAP_CTRL

- msp_ENDPOINT_RTPFDX_IFRAME_NOTIFY_CTRL

- msp_ENDPOINT_RTPFDX_OUT_OF_BAND_DCI

- msp_ENDPOINT_RTPFDX_RTP_PKTSZ_CTRL

- msp_ENDPOINT_RTPFDX_SET_VID_SKEW

- msp_ENDPOINT_RTPFDX_SET_VID_TX_PID

- msp_FILTER_JITTER_VID_LATENCY

## Structure for querying the video jitter buffer

Use the msp_FILTER_JITTER_VIDEO_STATE structure to get the status of the video jitter buffer.

## Structure for querying the H.264 video endpoint

Use the msp_ENDPOINT_RTPFDX_H264_TX_STATUS structure to get the transmit status of an H.264 video endpoint.