# msp_FILTER_JITTER_VID_LATENCY

This video-specific structure sets a video jitter buffer latency value.

Use this structure with the MSP_CMD_JITTER_CHG_VIDEO_LATENCY command, which is described in Setting the video jitter buffer latency.

#### Definition

typedef struct tag_msp_JITTER_VID_LATENCY
{
DWORD value;
} msp_FILTER_JITTER_VID_LATENCY;

#### Fields

Field name | Default | Description
--- | --- | ---
value | 0 | Video jitter buffer latency duration in ms. Valid values are 0 - 2000.