# msp_ENDPOINT_RTPFDX_RTTS_CTRL

This video-specific structure enables or disables RTTS for MPEG-4, H.263, and H.264 endpoints.

Use msp_ENDPOINT_RTPFDX_RTTS_CTRL with the MSP_CMD_RTPFDX_RTTS_CTRL command, which is described in Configuring real-time timestamp generation.

#### Definition

typedef struct
{
U32 enable; // NZ=enable, Z=disable
} msp_ENDPOINT_RTPFDX_RTTS_CTRL;

#### Fields

Field name | Default | Description
--- | --- | ---
enable | 0 | Enables or disables the RTTS feature. Valid values are: 0 - Disables RTTS. Non-zero value – Enables RTTS.