# Installation summary

The following table summarizes the procedure for installing the hardware and software components:

Step | Description
--- | ---
1 | Ensure that your PC system meets the system requirements.
2 | Configure the AG 2000-BRI board.
3 | Install the AG 2000-BRI board into one of the computer's PCI bus slots.
4 | If there are multiple H.100 boards, connect the H.100 bus to your H.100 boards.
5 | Install Natural Access, which also installs the AG 2000-BRI board driver and runtime software.
6 | Add configuration information for each board to the NMS OAM database. For more information, refer to the NMS OAM System User's Manual.
7 | Direct the OAM service to start the boards. For more information, refer to Configuring and starting the system with oamsys and to the NMS OAM System User's Manual.
8 | Verify that the installation is operational.

Note: If your system is powered down, you can install the board before you install the software. It does not matter if you install the board or the software first.

## AG driver software

The following drivers for operating AG boards are installed with Natural Access software:

Operating system | Driver names
--- | ---
Windows | aghw ag agsw ag95sw
UNIX | aghw agsw ag95sw agmx