# Default connections

If a board is configured for standalone operation (Clocking.HBus.ClockMode = STANDALONE), the DSPs and trunks are connected as shown in the following table.

Switch connection | MVIP-95
--- | ---
Full duplex connection between line interface voice information and DSP resources. | local:0:0..7 => local:5:0..7 local:4:0..7 => local:1:0..7

To change this default routing so the board can interoperate with other boards connected to it over the H.100 bus, disable the automatic routing by setting SwitchConnections = NO. When the bus is enabled (Clocking.HBus.ClockMode is not equal to STANDALONE), there is no default routing unless you set SwitchConnections = YES.