# Retrieving AG board configuration information: boardinf

boardinf is a program that reports the board number, address, type, number of ports, memory, and DSP timeslot assignments for each board in a system.

boardinf opens the AG driver and retrieves the configuration information for up to 16 AG 2000-BRI boards. If an AG 2000-BRI board exists and is properly initialized, its configuration is displayed and its DSP port addresses are displayed as one or more timeslot ranges.

To run boardinf:

Step | Action
1 | Ensure that the AG 2000-BRI boards were initialized.
2 | Open a command window.
3 | Enter the following command: boardinf boardinf displays the configuration information for each AG 2000-BRI board in the system that has been loaded and initialized.
4 | If no boards are detected, verify that the AG 2000-BRI board(s) has been loaded and initialized and repeat the command. If the AG 2000-BRI board configuration information is not as expected, review the board keyword file.