# Verifying the board installation

Complete the following steps to verify that the board is installed correctly:

Step | Action
1 | Create a board keyword file to boot an AG 2000-BRI board by copying or editing one of the sample board keyword files to match your specific configuration. Refer to Using board keyword files for more information. For example, use the agpi2bri.cfg file to configure the board for the Euro ISDN protocol.
2 | Run oammon to monitor the status of all boards.
3 | Use the pciscan utility to determine the bus and slot number. For more information about pciscan, refer to the NMS OAM System User's Manual.
4 | Edit the oamsys.cfg file to reflect the board locations in your system.
5 | Boot the board using the command: oamsys