# VoiceIdleCode

Sets the voice bit pattern transmitted by an idle DSP or to an unconnected line interface.

#### Syntax

VoiceIdleCode = voice_idlecode

#### Access

Read/Write

#### Type

Integer

#### Default

If Xlaw = MU-LAW, default = 0x7f.

If Xlaw = A-LAW, default = 0xd5.

#### Allowed values

0x00 - 0xFF

#### Example

VoiceIdleCode = 0xd5

#### Details

In general, a DSP is considered to be idle when no application is using it.

On digital trunks, the idle code is determined by local regulations and should not be altered.

#### See also

SignalIdleCode