# SignalIdleCode

Specifies the signal bit patterns transmitted by an idle DSP or to an unconnected line interface. In general, a DSP is considered to be idle when no application is using it.

#### Syntax

SignalIdleCode = signal_idlecode

#### Access

Read/Write

#### Type

Integer

#### Default

If Xlaw = MU-LAW, default = 0.

If Xlaw = A-LAW, default = 9.

#### Allowed values

0x00 - 0xFF

#### Example

SignalIdleCode = 0xd

#### See also

VoiceIdleCode