# MaxChannels

Specifies the maximum number of channels to allocate on the board.

#### Syntax

MaxChannels = numChannels

#### Access

Read/Write

#### Type

Integer

#### Default

8

#### Allowed values

1 - 255

#### Example

MaxChannels = 128

#### Details

The number of channels affects memory requirements. If Buffers[0].Num is not configured, two buffers are allocated per channel.

#### See also

Buffers[x].Num