# Hdlc[x].Boot

Enables or disables the HDLC channel associated with a particular trunk.

#### Syntax

Hdlc[x].Boot = boot

x = 0-(n-1) (0-based trunk number or range of trunk numbers where n equals the number of trunks on the board.)

#### Access

Read/Write

#### Type

String

#### Default

NO

#### Allowed values

YES | NO

#### Example

Hdlc[0..7].Boot = YES

#### See also

Hdlc[x].RxTimeSlot, Hdlc[x].TxTimeSlot