# General hardware specifications

This topic presents selected specifications of the CG 6060C board:

- Physical

- Media stream DSP processing

- IP network connectivity

- PSTN network connectivity

- Intra-chassis connectivity

- Software environment

- Host interface

- H.110 compliant interface

- Environment

- Power requirements

## Physical

Form factor | 6U CompactPCI per PICMG 2.0
PCI bus | 32 bit 33 or 64 MHz PCI bus
T1/E1 input/output | Through a rear I/O transition board
Ethernet input/output | Through a rear I/O transition board or PICMG 2.16 backplane
Board weight | Main board: 0.75 lb (0.36 kg) Rear I/O transition board: 0.55 lb (0.24 kg)

## Media stream DSP processing

Processors | There are a variety of configurations available for the CG 6060C board. The DSPs are Texas Instruments TMS320C5441s. There are four cores per DSP. Each DSP core executes 133 MIPS.
Capacity | Up to 120 ports of universal port media processing. Up to 480 ports of channel associated signaling.

## IP network connectivity

Physical | Dual 10/100Base-T Ethernet interfaces
Protocols | ARP ICMP IPSec IPv4 IPv6 RTP/RTCP UDP

## PSTN network connectivity

Physical | Four-trunk variant: T1/E1 with four RJ-48C interfaces on rear I/O transition board Eight-trunk variant: T1/E1 with eight RJ-48C interfaces on rear I/O transition board Eight-trunk variant: T1/E1 with one Dialogic® MD1 RJ-21 interface on a rear I/O transition board Sixteen-trunk variant: T1/E1 with two Dialogic® MD1 RJ-21 interfaces on rear I/O transition board
Protocols | ISDN CAS
Capacity | Up to 480 ports
Approvals | Refer to www.dialogic.com/declarations/default.htm for a list of countries where Dialogic has obtained approval for the board.

## Intra-chassis connectivity

Physical | H.110 CT bus on J4
Controller | Proprietary TSI

## Software environment

Development environment | NaturalAccess
Hot Swap | Per PICMG 2.1
Operating system | Windows UNIX Red Hat Linux

## Host interface

Feature | Specification
--- | ---
Electrical | CompactPCI bus designed to CompactPCI PICMG specification revision 2.1.
Mechanical | Designed to the CompactPCI PICMG specification revision 2.1 for 6U style cards.
Maximum number of ports per chassis | Limited by host processor resources.
I/O | PCI bus master/slave with DMA.
Addresses/interrupts | Address and interrupts automatically configured by CompactPCI BIOS (no jumpers or switches).
Plug and Play | Compatible on Windows.

## H.110 compliant interface

- Flexible connectivity between T1/E1 trunks, DSPs, and H.110 bus

- Switchable access to any of 4096 H.110 timeslots

- H.110 clock master or clock slave (software-selectable)

- Compatible with any H.110-compliant telephony interface

## Environment

Feature | Description
--- | ---
Operating temperature | 0 to 50 ° C
Storage temperature | -20 to 70 ° C
Humidity | 5 to 80%, non-condensing

## Power requirements

Board model | +3.3 V current requirement | +5 V current requirement | +12 V current requirement
CG 6060C/16-2L/4 TE | active: 2.13 A maximum reset: 0.84 A maximum | active: 0.72 A maximum reset: 0.47 A maximum | active and reset: 0.1 A maximum
CG 6060C/32-2L/4 TE | active: 2.21 A maximum reset: 0.94 A maximum | active: 0.89 A maximum reset: 0.60 A maximum | active and reset: 0.1 A maximum
CG 6060C/42-2L/4 TE | active: 2.25 A maximum reset: 0.99 A maximum | active: 0.98 A maximum reset: 0.66 A maximum | active and reset: 0.1 A maximum
CG 6060C/11-2L/8 TE | active: 2.32 A maximum reset: 0.76 A maximum | active: 0.64 A maximum reset: 0.32 A maximum | active and reset: 0.1 A maximum
CG 6060C/21-2L/8 TE | active: 2.46 A maximum reset: 0.91 A maximum | active: 0.80 A maximum reset: 0.54 A maximum | active and reset: 0.1 A maximum
CG 6060C/11-2L/16 TE | active: 3.36 A maximum reset: 0.79 A maximum | active: 0.65 A maximum reset: 0.33 A maximum | active and reset: 0.1 A maximum
CG 6060C/21-2L/16 TE | active: 3.49 A maximum reset: 0.94 A maximum | active: 0.81 A maximum reset: 0.55 A maximum | active and reset: 0.1 A maximum
CG 6060C/42-2L/16 TE | active: 3.57 A maximum reset: 1.05 A maximum | active: 0.99 A maximum reset: 0.67 A maximum | active and reset: 0.1 A maximum