# IPv6.Link[x].EnablePing

Enables or disables IPv6 PING on the specified Ethernet interface.

#### Syntax

IPv6.Link[x].EnablePing = mode

x = index of the link entry

#### Access

Read/Write

#### Type

String

#### Default

YES

#### Allowed values

YES | NO

#### Example

IPv6.Link[1].EnablePing = YES

#### Details

By default, PING is enabled for IPv6 Ethernet interfaces. For more information, refer to Configuring IPv6 Ethernet connections.

#### See also

IPv6.Link[x].Enable, IPv6.Link[x].IPSec