# IPC.AddRoute[x].VlanTag

Specifies a VLAN tag to be added to all packets sent to the IPv4 subnet specified by the address and mask in IPC.AddRoute[x].DestinationAddress and IPC.AddRoute[x].Mask.

#### Syntax

IPC.AddRoute[x].VlanTag = tag

x = index of the route entry

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

0 - 4094

#### Example

IPC.AddRoute[1].VlanTag = 5

#### Details

A VLAN tag is not valid with route definitions (GatewayAddress must not be set.)

For more information, refer to Configuring IPv4 Ethernet connections.

#### See also

IPC.AddRoute[x].Interface, IPC.AddRoute[x].Mask