# TPKT.ComplexRxPort

Specifies a UDP port number on which to receive complex ThroughPacket packets.

#### Syntax

TPKT.ComplexRxPort = portnumber

#### Access

Read/Write

#### Type

Integer

#### Default

None.

#### Allowed values

A valid UDP port number.

#### Example

TPKT.ComplexRxPort = 49152

#### Details

For information about the Clarent ThroughPacket multiplexing algorithm and its implementation in the Fusion API, refer to the Dialogic® NaturalAccess™ Fusion™ VoIP API Developer’s Manual.

#### See also

TPKT.ComplexForward.Count, TPKT.ComplexForward[x].DestinationPacketSize, TPKT.ComplexForward[x].LifeTimeTicks, TPKT.ComplexTxPort, TPKT.NumberOfComplexForwardConditions