# IPv6.Link[x].ICMPRateLimit

Specifies the IPv6 ICMP rate limit for the specified Ethernet interface.

#### Syntax

IPv6.Link[x].ICMPRateLimit = icmplimit

x = index of the link entry

#### Access

Read/Write

#### Type

String

#### Default

100

#### Allowed values

0 - 9999

#### Example

IPv6.Link[1].ICMPRateLimit = 5250

#### Details

For information about ICMP, refer to RFC 2463 Internet Control Message Protocol (ICMPv6) for the Internet Protocol Version 6 (IPv6). For information about using board keywords to configure IPv6 Ethernet interfaces, refer to Configuring IPv6 Ethernet connections.

#### See also

IPv6.Link[x].HopLimit, IPv6.Link[x].NDAttempts