# ConferencingStream.SlotCount

Specifies the number of logical timeslots allocated to logical conferencing streams 68 and 69.

#### Syntax

ConferencingStream.SlotCount = slotcount_number

#### Access

Read/Write

#### Type

Integer

#### Default

128

#### Example

ConferencingStream.SlotCount = 128

#### Allowed values

0 - 1500

#### Details

The number of reserved timeslots varies by user configuration. Refer to the Dialogic® NaturalAccess™ NaturalConference™ API Developer’s Manual for more information about conferencing. For information about streams and timeslots on CG boards, refer to the CAS mode switch model, the PRI mode switch model, and the RAW mode switch model.

#### See also

ConferencingStream.Enable