# CG 6060C board features

The CG 6060C board is a CompactPCI Media Board. It is a high-density platform for IVR, fax, VoIP, and media server applications. The board uses a high performance PowerPC processor.

Configurations with a main board and attached daughterboard provide up to 16 T1 or E1 digital trunk interfaces and two Ethernet 10/100Base-T interfaces.

Refer to www.dialogic.com/declarations/default.htm for a list of available CG 6060C board configurations, for a list of countries where Dialogic has obtained approval for the CG 6060C board, and for product updates.

CG 6060C boards include the following features:

- DSP resources

  The CG 6060C board has up to 4,256 MIPS of media processing DSPs.

- CompactPCI bus connectivity

  Each CG 6060C board is designed to reside in a single CompactPCI bus slot. Each board contains a 5-volt CompactPCI bus interface compliant with the CompactPCI Specification PICMG 2.0 R2.1. The CompactPCI interface is a 33 MHz, 32-bit master/target device.

- Trunk connectivity

  Board configurations provide up to 16 T1 or E1 network interfaces for digital trunk connectivity through a rear I/O transition board (if the board is equipped with trunk interfaces). You must configure the board for either T1 or E1. For more information, refer to Configuring the T1 or E1 interface and to NetworkInterface.T1E1[x].Type.

- H.110 bus connectivity

  The CG 6060C board fully supports the H.110 bus specification. The H.110 bus enables multiple boards to share data. For example, you can connect two or more CG 6060C boards for applications that perform trunk-to-trunk switching. You can use H.110 compatible products from other manufacturers with the CG 6060C board.

- Telephony bus switching

  Switching for the CG 6060C board offers support for the H.110 bus within the H.110 architecture. On the CG 6060C board, switch connections are allowed for a total of 1024 full duplex connections between local devices and the H.110 bus.

- Ethernet connectivity

  The CG 6060C board contains two 10/100Base-T Ethernet connections through a rear I/O transition board for fast Ethernet connectivity and support of both IPv4 and IPv6. For more information, refer to Connecting to an Ethernet network.

- PowerPC Microprocessor (A MCC 405 EP)

  The PowerPC Microprocessor is a high performance 333 MHz RISC processor.

- Flash memory

  8 MB of available flash memory is available on the board.

The following illustration shows where various components are located on a CG 6060C board: