# Installation summary

The following table summarizes the procedure for installing the hardware and software components:

Step | Action
--- | ---
1 | Ensure that your PC system meets the system requirements.
2 | Power down the system if it is running.
3 | Install the rear I/O transition board in a CompactPCI bus slot.
4 | If necessary, configure the DIP switches.
5 | If necessary, configure the T1 or E1 interface.
6 | Install the CG 6060C board into the corresponding slot in the front of the chassis.
7 | Power up the system.
8 | Install NaturalAccess, which also installs the CG board driver, runtime software, and the hardware interface drivers.
9 | For each board, create a board keyword file that details the board configuration settings. Find the closest example file in \nms\cg\cfg and use it as a baseline.
10 | Create a system configuration file that identifies all boards in the system and their associated board keyword files. For more information, refer to Configuring and starting the system with oamsys and to the Dialogic® NaturalAccess™ OAM System Developer’s Manual.
11 | Run oamsys to configure the boards as specified in the configuration files.
12 | Verify that the installation is operational.