# Installation summary

The following table summarizes the procedure for installing the hardware and software components:

Step | Action
--- | ---
1 | Ensure that your PC system meets the system requirements.
2 | Power down the system if it is running.
3 | Install the rear I/O transition board in a CompactPCI bus slot.
4 | If necessary, configure the DIP switches.
5 | Install the CG 6565C board into the corresponding slot in the front of the chassis.
6 | Power up the system.
7 | Install NaturalAccess, which also installs the CG board driver and runtime software. Note: The hardware interface drivers are installed with NaturalAccess software.
8 | Create or edit an OAM API system configuration file and board keyword file describing your setup. For more information, refer to Configuring and starting the system with oamsys and to the Dialogic® NaturalAccess™ OAM System Developer’s Manual.
9 | Run oamsys to configure the boards as specified in the configuration files.
10 | Connect the board interfaces to T1 or E1 trunks and Ethernet connections.
11 | Verify that the installation is operational.