# TPKT.Enable

Enables or disables ThroughPacket packet multiplexing functionality on the board.

#### Syntax

TPKT.Enable = value

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

0 | 1

#### Example

TPKT.Enable = 1

#### Details

Set TPKT.Enable to 1 to enable ThroughPacket multiplexing. Set TPKT.Enable to 0 to disable ThroughPacket multiplexing.

On systems where ThroughPacket multiplexing is enabled, a DLMFiles[x] keyword must also be set to cg6ktpkt so that the ThroughPacket runtime component is transferred to the board.

For information about the Clarent ThroughPacket multiplexing algorithm and its implementation in Fusion software, refer to the Dialogic® NaturalAccess™ Fusion™ VoIP API Developer’s Manual.

#### See also

TPKT.ComplexRxPort, TPKT.ComplexTxPort