# ConferencingStream.SlotCount

Specifies the number of logical timeslots allocated to logical conferencing streams 68 and 69.

#### Syntax

ConferencingStream.SlotCount = slotcount_number

#### Access

Read/Write

#### Type

Integer

#### Default

128

#### Example

ConferencingStream.SlotCount = 128

#### Allowed values

0 - 1500

#### Details

The number of reserved timeslots varies by user configuration. Refer to the Dialogic® NaturalAccess™ NaturalConference™ API Developer’s Manual for more information about conferencing. For information about streams and timeslots on CG boards, refer to CAS mode switching, PRI mode switching, and RAW mode switching.

#### See also

ConferencingStream.Enable