# Editable keywords

The following table summarizes the keywords that are editable:

If you want to... | Use these keywords...
--- | ---
Specify information about the board | AutoStart AutoStop EnableMonitor MaxChannels Name Number
Specify the warning threshold for the fan tachometer | FanTach.WarnThres
Specify CG 6565E line interfaces as T1 or E1 | NetworkInterface.T1E1[x].Type
Set up trunk information for the board | NetworkInterface.T1E1[x].FrameType NetworkInterface.T1E1[x].Impedance NetworkInterface.T1E1[x].Length NetworkInterface.T1E1[x].LineCode NetworkInterface.T1E1[x].SignalingType NetworkInterface.T1E1[x].Type NetworkInterface.T1E1[x].CRCMFMode
Set up trunk information specific to ISDN | NetworkInterface.T1E1[x].D_Channel NetworkInterface.T1E1[x].ISDN.D_Channel_Backup_Trunk NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Board NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].NAI NetworkInterface.T1E1[x].ISDN.NFAS_Member[y].Trunk NetworkInterface.T1E1[x].ISDN.NFASGroup
Modify memory allocation | Buffers[x].Size DynamicRecordBuffers
Set IPv4 addressing and static IPv4 routing table information for the board | IPC.AddRoute[x].DestinationAddress IPC.AddRoute[x].GatewayAddress IPC.AddRoute[x].Interface IPC.AddRoute[x].Mask IPC.AddRoute[x].VlanTag
Set IPv6 addressing for the board | IPv6.Link[x].Enable IPv6.Link[x].EnablePing IPv6.Link[x].HopLimit IPv6.Link[x].ICMPRateLimit IPv6.Link[x].IPSec IPv6.Link[x].MTU IPv6.Link[x].NDAttempts IPv6.Link[x].NDReachabilityTimer IPv6.Link[x].NDRetranTimer
Set up clocking information | Clocking.HBus.ClockMode Clocking.HBus.ClockSource Clocking.HBus.ClockSourceNetwork
Configure clock fallback | Clocking.HBus.AutoFallBack Clocking.HBus.FallBackClockSource Clocking.HBus.FallBackNetwork
Set up clocking information specific to NETREF | Clocking.HBus.NetRefSource Clocking.HBus.NetRefSourceNetwork Clocking.HBus.NetRefSpeed Clocking.HBus.SClockSpeed Clocking.HBus.Segment
Set up switching information | SwitchConnections SwitchConnectMode DSPStream.SlotCount DSPStream.SignalIdleCode[x] DSPStream.VoiceIdleCode[x]
Enable conferencing streams for switching | ConferencingStream.Enable ConferencingStream.SlotCount
Manage the DSP resources on the board | Resource[x].Definitions Resource[x].DSPs Resource[x].Name Resource[x].Size Resource[x].StartTimeSlot Resource[x].TCPs
Set up debug level information | DebugMask EnableMonitor
Configure HDLC signaling | Hdlc[x].Boot Hdlc[x].RxTimeSlot Hdlc[x].TxTimeSlot
Configure DSPs | DSP.C5x[x].CmdQSize DSP.C5x[x].CmdQStart DSP.C5x[x].DataInQSize DSP.C5x[x].DataInQStart DSP.C5x[x].DspOutQSize DSP.C5x[x].DspOutQStart DSP.C5X[x].Image DSP.C5x[x].Libs[y] DSP.C5x[x].NumRxTimeSlots DSP.C5x[x].NumTxTimeSlots DSP.C5x[x].OS DSP.C5x[x].XLaw
Control switching on the echo canceler reference stream | Echo.AutoSwitchingRefSource Echo.EnableExternalPins
Specify the board location | Location.PCI.Bus Location.PCI.Slot
Implement ThroughPacket packet multiplexing | TPKT.ComplexForward.Count TPKT.ComplexForward[x].DestinationPacketSize TPKT.ComplexForward[x].LifeTimeTicks TPKT.ComplexRxPort TPKT.ComplexTxPort TPKT.Enable TPKT.NumberOfComplexForwardConditions TPKT.SimpleRxPort TPKT.SimpleTxPort
Modify the hardware echo cancellation settings | HardwareEcho.EchoChipEnabled HardwareEcho.Trunk[x].OnOffTimeslots HardwareEcho.XLaw