# Clocking.HBus.Segment

Specifies the CT bus segment to which the board is connected. In most cases, the chassis contains only one segment.

For more information about setting up CT bus clocking and about the rules and restrictions that apply to setting up clocking with CG 6565E boards, refer to Configuring board clocking.

#### Syntax

Clocking.HBus.Segment = number

#### Access

Read/Write

#### Type

Integer

#### Default

1

#### Allowed values

Positive integer

#### Example

Clocking.HBus.Segment = 1

#### See also

Clocking.HBus.SClockSpeed