# Location.PCI.Slot

Defines the logical slot location of the board on the PCI bus.

#### Syntax

Location.PCI.Slot = slotnum

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Example

Location.PCI.Slot = 5

#### Allowed values

0 - 9999

#### Details

A PCI bus and slot number identifies every slot in the system. Identify a board by specifying its bus and slot number.

A PCI board's address and interrupt is automatically set by the system. This statement along with Location.PCI.Bus assigns the board number to the physical board.

pciscan can be used to determine the PCI bus and slot assigned for all NaturalAccess PCI and PCIe boards in the system. Refer to the Dialogic® NaturalAccess™ OAM System Developer’s Manual for information about pciscan.

Note: The Slot setting in the oamsys system configuration file overrides this keyword.

Location.PCI.Slot is mandatory for PCI and PCIe boards.