# Name

Specifies the name assigned to the CG 6565E board.

#### Syntax

Name = board_name

#### Access

Read/Write

#### Type

String

#### Default

CG_6000C

#### Allowed values

String up to 64 characters long.

#### Example

Name = Brd1

#### Details

This setting is assigned by the OAM Supervisor if the user does not specify a name in the system configuration file. This setting is guaranteed to be unique within the chassis.

#### See also

Number