# DebugMask

Specifies the type and level of tracing that the board performs.

#### Syntax

DebugMask = mask

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

A value shown in the following table.

#### Example

DebugMask = 0x00000200

#### Details

To view the results of CG 6565 tracing, you must be running oammon.

You can specify the following DebugMask parameters:

Value | Description
--- | ---
0x00000001 | Additional initialization messages.
0x00000002 | Legacy initialization messages.
0x00000008 | Total resources for each DSP and calculate resource string.
0x00000100 | Host interface up and down messages.
0x00000200 | Inter-manager messages.
0x00000400 | All manager messages.
0x00000800 | High speed memory usage tracing messages.
0x00001000 | Memory usage tracing messages while rechecking allocated usage.
0x00002000 | Framers global tracing level.
0x00004000 | General clock tracing messages.
0x80000000 | Available memory.