# Informational keywords

This topic describes read-only keywords for retrieving information. Do not edit the keywords listed in this topic. Use these keywords for retrieving information about the:

- Board

- Driver

- Miscellaneous board information

- EEPROM

## Retrieving board information

Keyword | Type | Description
--- | --- | ---
State | String | State of the physical board.

## Retrieving driver information

Keyword | Type | Description
--- | --- | ---
Driver.BoardID | Integer | Number used by the CG board driver to refer to this board. Two boards accessed by different drivers can have the same driver ID number.
Driver.Name | String | Operating system independent name (the root name) of the board driver.
SwitchDriver.Name | String | Operating system independent name (the root name) of the board switching driver.

## Retrieving miscellaneous information

Keyword | Type | Description
--- | --- | ---
NetworkInterface.T1E1[x].ISDN.NFAS_Member.Count | Integer | Number of interfaces in this NFAS group. The value is calculated based on the number of T1E1[x].ISDN.NFAS_MEMBER[y] structures specified.
NetworkInterface.Ethernet[x].MAC_Address | String | Specifies the MAC address.

## Retrieving EEPROM information

The data type for all EEPROM keywords is Integer.

Keyword | Description
--- | ---
Eeprom.AssemblyRevision | Hardware assembly level.
Eeprom.ATETestBit | Indicates whether the ATE test was successful. A non-zero value indicates success.
Eeprom.DSPExtClk | Oscillator used to trigger the DSP.
Eeprom.DSPSpeed | DSP processor speed in MHz.
Eeprom.DSPType | Type of DSP on the board (for example, TI C5420).
Eeprom.EthernetType | Type of Ethernet connection on the board (for example, 10/100/1000Base-T).
Eeprom.Family | Family ID of the board.
Eeprom.FlashBlkSz | Size of the Flash.
Eeprom.FlashID | Type of Flash chip ID used on the board.
Eeprom.HostBusType | Type of host bus used on the board (for example, PCI).
Eeprom.MFGWeek | Week of the last full test.
Eeprom.MFGYear | Year of the last full test.
Eeprom.MSBType | Type of CT bus used on the board.
Eeprom.NumCPU | Number of CPUs on the board.
Eeprom.NumDaughterCard | Number of daughterboards attached to the main board.
Eeprom.NumDSPCores | Number of DSP cores on the board.
Eeprom.NumEthernet | Number of Ethernet connections on the board.
Eeprom.NumSwitch | Number of switches on the board.
Eeprom.NumTrunk | Number of PSTN line interfaces on the board.
Eeprom.Product | OAM product ID number associated with the board. This number is factory configured and unique to each board type. The product ID for the CG 6565 board is 0x635.
Eeprom.SerialNum | Board's serial number.
Eeprom.SoftwareCompatibility | Minimum software revision level.
Eeprom.SwitchType | Type of switch on the board (for example, T8100).
Eeprom.TrunkType | Type of line interfaces on the board (for example, digital).