# Installation summary

The following table summarizes the procedure for installing the hardware and software components:

Step | Action
--- | ---
1 | Ensure that your PC system meets the system requirements.
2 | Power down the system if it is running.
3 | If necessary, configure the CG 6565 board for H.100 bus termination.
4 | Install the CG 6565 board in a PCI bus slot.
5 | Power up the system.
6 | Install NaturalAccess, which also installs the CG board driver and runtime software. The hardware interface drivers are installed with NaturalAccess software.
7 | Create or edit an OAM API system configuration file and board keyword file describing your setup. For more information, refer to Configuring and starting the system with oamsys and the Dialogic® NaturalAccess™ OAM System Developer’s Manual.
8 | Configure the CG 6565 board either without trunk interfaces or with T1 or E1 interfaces.
9 | Configure an Ethernet connection. For more information, refer to the Configuring Ethernet interfaces section.
10 | Run oamsys to configure the boards as specified in the configuration files.
11 | Connect the board interfaces to T1 or E1 trunks (if enabled) and Ethernet connections.
12 | Verify that your installation is operational.