# Connecting to an Ethernet network

To connect a CG 6565 board to an Ethernet network, insert a Category 5 shielded twisted pair (STP) cable into one or both of the board's Ethernet connectors.

To set up IPv4 or IPv6 connections, specify appropriate keyword settings in the board keyword file. For more information, refer to Configuring IPv4 Ethernet connections or Configuring IPv6 Ethernet connections.