# Clocking.HBus.Segment

Specifies the CT bus segment to which the board is connected. In most cases, the chassis contains only one segment.

For information about setting up CT bus clocking, and rules and restrictions for configuring CT bus clocking, refer to Configuring board clocking.

#### Syntax

Clocking.HBus.Segment = speed

#### Access

Read/Write

#### Type

Integer

#### Default

1

#### Allowed values

0 to 65535

#### Example

Clocking.HBus.Segment = 1

#### See also

Clocking.HBus.SClockSpeed