# BootDiagnosticLevel

Specifies the level of diagnostics performed during initialization of the board. When disabled (set to 0) the board ignores any diagnostic errors returned while it is being initialized.

#### Syntax

BootDiagnosticLevel = level

#### Access

Read/Write (plug-in level)

#### Type

Integer

#### Default

1

#### Allowed values

-65535 to 65535

#### Example

BootDiagnosticLevel = 1

#### Details

The valid values for level are 0, and 1. Zero (0) indicates that no diagnostics are performed, and 1 is the maximum level.

If a test fails, the test number is reported back as the error code.

Note: Some tests can pass back more than one error code, depending on the options selected and/or the mode of failure.

You must be running oammon to view diagnostic results.