# DebugMask

Specifies the type and level of tracing that the board performs.

#### Syntax

DebugMask = mask

#### Access

Read/Write

#### Type

Integer

#### Default

0

#### Allowed values

mask = Any value shown in the following table.

#### Example

DebugMask = 0x00000200

#### Details

You can specify the following DebugMask parameters:

Value | Description
--- | ---
0x00000001 | Additional initialization messages.
0x00000002 | Legacy initialization messages.
0x00000004 | DLM download and start address.
0x00000008 | Total resources for each DSP.
0x00000080 | DLM resolving and relocation.
0x00000100 | Host interface up and down messages.
0x00000200 | Inter-manager messages
0x00000400 | All manager messages.
0x80000000 | Available memory.
0xFFFFFFFF | All of the above.

DebugMask settings takes effect immediately. It is not necessary to reboot the board for these settings to take effect.