# AutoStop

Specifies whether the board automatically stops when ctdaemon is stopped.

#### Syntax

AutoStop = argument

#### Access

Read/Write

#### Type

String

#### Default

NO

#### Allowed values

YES | NO

#### Example

AutoStart = NO

#### Details

The Supervisor keyword AutoStopEnabled enables or disables the autostop feature. If AutoStopEnabled is set to YES, the Supervisor stops each board whose AutoStop keyword is set to YES when ctdaemon is stopped. If AutoStopEnabled is set to NO, no boards are stopped automatically, regardless of the setting of the AutoStop keyword.

For details, refer to the NMS OAM System User's Manual.

#### See also

AutoStart