# Booting CG boards

To boot a CG board:

Step | Action
1 | Edit one of the sample Fusion CG board keyword files to specify settings appropriate for the system.
2 | Edit the fusion_oamsys.cfg file by specifying the following:
Entry | Description
Bus | Bus number of the CG board.
Slot | Slot number of the CG board
File | File name of the CG board keyword file (for example, cg6kfusion-t.cfg or cg6kfusion-e.cfg).
You can obtain the CG board bus and slot number by running the pciscan utility.
3 | Enter the following at the command prompt: oamsys -f

For more information about using OAM board configuration tools and pciscan, refer to the Dialogic® NaturalAccess™ OAM System Developer’s Manual.